UBC Rapid

Bernhard: Progress and To Do

|  |  |  |
| --- | --- | --- |
| 19 Feb 2011 | Progress made | To do |
|  | * Detached C and B sections * Cleaned and sorted parts * Identified current bearing types (Thomson | * Part B0002 is corroded and will need either replacement or treatment: Prepare parts drawings * Can mill down top 1mm surface and coat with a new running surface * Get new belts and pulleys: Spec current ones * Modify axis A to work with leadscrew? * Modify axis C for direct drive: Motor mount to B0001 * Requires solidworks models of entire A and B axis setup |
|  |  |  |
|  |  |  |